How to run:

1. Calibrate camera
2. Run video on ORBSLAM3 and save output
3. Go to aruco\_try and type the mp4 location file, you can run to see if the aruco part works well
4. Go to slam preprocess, make sure the SLAM output is saved in the right place run it.
5. Go to main\_new\_new\_new , run it.